No.585 USB UPDATE PROCEDURE

1. Turn off power to the No585.

2. Copy the bundle update file to a USB flash drive (FAT32 format) and insert it into the USB port on the back of the unit.  (If the file is in the ZIP format, be sure to unzip it first then copy the contents to the drive).  

3. Power up the No585.  Wait for the system to fully power on and enter standy mode.

4. Press the standby button to bring the No585 out of Standby.

5. Press the setup button then navigate using the input control knob to:
Advanced -> 
	Firmware -> Update=USB 
and press the enter button. 

6. You will see "Update=USB" with a flashing equals sign on the display indicating that you can select the method for upgrade (USB or ENET).  Press enter again to select USB. 

NOTE: DO NOT REMOVE THE USB DRIVE OR INTERRUPT POWER DURING THE UPDATE PROCESS.

7. The No585 will check the drive for a valid update package - if a valid update is found, it will proceed with the installation.  You may see a message on the display indicating that the process could take more than 30 minutes (in some cases updating can take 30 minutes or less).  

8. When the update process is complete the unit will display "Update complete - Cycle Power Now".   Turn off power to the No585 then remove the USB drive before re-applying power.  

9.  After powering on, verify that the update completed properly by pressing the standby button, then press the setup button and navigate to:
Advanced ->
	Firmware -> Ver=1.13/1.09 
